**TECHNICAL DATA**

|  |  |
| --- | --- |
| **Jaguar XE 2.0 Diesel 163** | |
| **ENGINE & TRANSMISSION** | |
| Engine capacity (cc) | 1,999 |
| Cylinders | 4 in-line |
| Valves per cylinder | 4; DOHC |
| Bore/ stroke (mm) | 83.0/ 92.4 |
| Compression ratio | 15.5:1 |
| Fuel injection system | 1,800bar common rail |
| Boosting system | Single variable geometry turbo |
| Power PS (kW) | 163 (120) @ 4,000rpm |
| Torque Nm (lb ft) | 380 (280) @ 1,750-2,500rpm |
| Transmission | ZF 8HP45 8-speed automatic,  6-speed manual |
| **PERFORMANCE & FUEL ECONOMY** | |
| 0-60mph (sec) | 7.9 [man] / 7.7 [auto] |
| 0-100km/h (sec) | 8.4 [man] / 8.2 [auto] |
| Top speed mph (km/h) | 141 (227) [man]\* / 141 (227) [auto]\* \*UK only: 132 (212) |
| Fuel consumption mpg (litres/100km) EU combined | 75.0(3.8) [man] / 71.7 (3.9) [auto] |
| CO2 emissions (g/km) EU combined cycle | 99 [man] / 104 [auto] |
| **DIMENSIONS & VOLUMES** | |
| Length (mm) | 4,672 |
| Width inc./ excl. mirrors (mm) | 2,075/ 1,850 |
| Height (mm) | 1,416 |
| Wheelbase (mm) | 2,835 |
| Track front/ rear (mm) | 1,607/ 1,608 |
| Kerbweight (kg) | From 1,474 [man] / 1500 [auto] |
| Boot volume (litres) | 450 / 455 [no spare] |
| Fuel tank capacity (usable) litres | 47 |

|  |  |
| --- | --- |
| **Jaguar XE 2.0 Diesel 180** | |
| **ENGINE & TRANSMISSION** | |
| Engine capacity (cc) | 1,999 |
| Cylinders | 4 in-line |
| Valves per cylinder | 4; DOHC |
| Bore/ stroke (mm) | 83.0/ 92.4 |
| Compression ratio | 15.5:1 |
| Fuel injection system | 1,800bar common rail |
| Boosting system | Single variable geometry turbo |
| Power PS (kW) | 180 (132) @ 4,000rpm |
| Torque Nm (lb ft) | 430 (317) @ 1,750-2,500rpm |
| Transmission | ZF 8HP45 8-speed automatic,  6-speed manual |
| **PERFORMANCE & FUEL ECONOMY** | |
| 0-60mph (sec) | 7.4 [man] / 7.4 [auto] |
| 0-100km/h (sec) | 7.8 [man] / 7.8 [auto] |
| Top speed mph (km/h) | 142 (228) [man]\* / 142 (228) [auto]\* \*UK only: 140 (225) |
| Fuel consumption mpg (litres/100km) EU combined | From 67.3 (4.2) [man]/ 67.3 (4.2) [auto] |
| CO2 emissions (g/km) EU combined cycle | From 109 [man]/ 109 [auto] |
| **DIMENSIONS & VOLUMES** | |
| Length (mm) | 4,672 |
| Width inc./excl. mirrors (mm) | 2,075/ 1,850 |
| Height (mm) | 1,416 |
| Wheelbase (mm) | 2,835 |
| Track front/ rear (mm) | 1,602/ 1,603 |
| Kerbweight (kg) | From 1,550 [man] / 1,565 [auto] |
| Boot volume (litres) | 450 / 455 [no spare] |
| Fuel tank capacity (usable) litres | 56 |

|  |  |
| --- | --- |
| **Jaguar XE 2.0 Petrol 200** | |
| **ENGINE & TRANSMISSION** | |
| Engine capacity (cc) | 1,999 |
| Cylinders | 4 in-line |
| Valves per cylinder | 4; DOHC |
| Bore/ stroke (mm) | 87.5/ 83.1 |
| Compression ratio | 10.0:1 |
| Fuel injection | 150bar direct injection |
| Boosting system | Single monoscroll turbocharger |
| Power PS (kW) | 200 (147) @ 5,500rpm |
| Torque Nm (lb ft) | 280 (206) @ 1,750-4,000rpm |
| Transmission | ZF 8HP45 8-speed automatic |
| **PERFORMANCE** | |
| 0-60mph (sec) | 7.1 |
| 0-100km/h (sec) | 7.7 |
| Top speed mph (km/h) | 147 (237) |
| Fuel consumption mpg (litres/100km) EU combined | 37.7 (7.5) |
| CO2 emissions (g/km) EU combined cycle | 179 |
| **DIMENSIONS** | |
| Length (mm) | 4,672 |
| Width inc./excl. mirrors (mm) | 2,075/ 1,850 |
| Height (mm) | 1,416 |
| Wheelbase (mm) | 2,835 |
| Track front/ rear (mm) | 1,602/ 1,603 |
| Kerbweight (kg) | From 1,530 |
| Boot volume (litres) | 450 / 455 [no spare] |
| Fuel tank capacity (usable) litres | 63 |

|  |  |
| --- | --- |
| **Jaguar XE 2.0 Petrol 240** | |
| **ENGINE & TRANSMISSION** | |
| Engine capacity (cc) | 1,999 |
| Cylinders | 4 in-line |
| Valves per cylinder | 4; DOHC |
| Bore/ stroke (mm) | 87.5/ 83.1 |
| Compression ratio | 10.0:1 |
| Fuel injection | 150bar direct injection |
| Boosting system | Single monoscroll turbocharger |
| Power PS (kW) | 240 (177) @ 5,500rpm |
| Torque Nm (lb ft) | 340 (250) @ 1,750-4,000rpm |
| Transmission | ZF 8HP45 8-speed automatic |
| **PERFORMANCE** | |
| 0-60mph (sec) | 6.5 |
| 0-100km/h (sec) | 6.8 |
| Top speed mph (km/h) | 155 (250) |
| Fuel consumption mpg (litres/100km) EU combined | 37.7 (7.5) |
| CO2 emissions (g/km) EU combined cycle | 179 |
| **DIMENSIONS** | |
| Length (mm) | 4,672 |
| Width inc./excl. mirrors (mm) | 2,075/ 1,850 |
| Height (mm) | 1,416 |
| Wheelbase (mm) | 2,835 |
| Track front/ rear (mm) | 1,602/ 1,603 |
| Kerbweight (kg) | From 1,535 |
| Boot volume (litres) | 450 / 455 [no spare] |
| Fuel tank capacity (usable) litres | 63 |

|  |  |
| --- | --- |
| **Jaguar XE 3.0 Petrol 340** | |
| **ENGINE & TRANSMISSION** | |
| Engine capacity (cc) | 2,995 |
| Cylinders | V6 |
| Valves per cylinder | 4; DOHC |
| Bore/ stroke (mm) | 84.5/ 89.0 |
| Compression ratio | 10.5:1 |
| Fuel injection | 150bar spray-guided direct injection |
| Boosting system | Twin-Vortex supercharger |
| Power PS (kW) | 340 (250) @ 6,500rpm |
| Torque Nm (lb ft) | 450 (332) @ 4,500rpm |
| Transmission | ZF 8HP45 8-speed automatic |
| **PERFORMANCE** | |
| 0-60mph (sec) | 4.9 |
| 0-100km/h (sec) | 5.1 |
| Top speed mph (km/h) | 155 (250) |
| Fuel consumption mpg (litres/100km) EU combined | 34.9 (8.1) |
| CO2 emissions (g/km) EU combined cycle | 194 |
| **DIMENSIONS** | |
| Length (mm) | 4,672 |
| Width inc./excl. mirrors (mm) | 2,075/1,850 |
| Height (mm) | 1,416 |
| Wheelbase (mm) | 2,835 |
| Track front/ rear (mm) | 1,602/ 1,603 |
| Kerbweight (kg) | From 1,665 |
| Boot volume (litres) | 450 / 455 [no spare] |
| Fuel tank capacity (usable) litres | 63 |

Figures are manufacturer’s estimates and are subject to certification